|  |  |
| --- | --- |
| **MODEL: STHT30AG30 - HOPPER TYPE SEMI-TRAILER** **Body / Chassis:**Manufactured from high-strength steel by using special submerged welding machines. Chassis, frame and backbone structure are suitable for heavy-loads and difficult site conditions and designed for esthetic appearance and durability.* Construction “Domex 700”
* Chassis “Domex 700”
* Goose-neck “Domex 700”
* Unloading hopper, “Domex 700”
* Upper filler caps ”Aluminum alloy”
* Hopper body “Aluminum alloy”
* Pneumatic botton unloading covers and mechanical safety locks

 **Axles:*** 3 axles, 12 ton capacity, square section

**Front Axle Lifting :** Operated from the cab, protracting the tire life-cycle.**King-Pin :** 2” bolt-connected in DIN Standards, interchangeable with 3.5”**Landing Legs :**  “S 2000 plus” model telescopic landing legs mechanical with two speeds, Dynamic: 25 000 kg,Static: 50 000 kg**Brake System :*** Dual circuit brake hardware
* 30” Service brake bellows
* 30x30” Emergency brake bellows
* Load balancing distribution valve
* Automatic brake adjusters
* EBS Brake System “WABCO”

**Suspension System :*** Air -suspension “5813”
* 100 mm Z-type springs
* “WABCO” suspension valves
* Shock Absorbers

**Electricity Hardware :*** 12/24 Volt Lighting System
* 7 pole distribution cable
* Electrical socket for lighting,
* 4 x 2 side lamps,
 | *<< All measures are declared with 2% margin >>* **Dimensions :** * Total Length : 10,890 mm
* Total width : 2.550 mm
* Ground height : 3.800 mm
* Tare Weight : 6,700 kg
* Capacity : 33 m3

**Tires :** Bridgestone - Pirelli - Good Year  385 / 65 R 22.5” size, 6+1 units tubeless tires and steel rims.**Painting :** All steel parts are painted with two layers of anti-corrosive primer coats and top acrylic colours.**Standard Accessories:** * 1 x spare tire holder
* FRP steel mudguards
* Aluminum ladder and barriers
* 1 x Tool box
* 1 x water tank “chrome nickel”
* Parking chock with handle.

**Optional:** * Aluminum wheels

REMARK : Our products are under 2 years local and one year international warranty against manufacturing defects.100_3727.JPGRequired hardware for traffic. |